Parameters Solar charge Controller
Nr
1 Analogue Range Start	
2 Analogue Range End	
3 Analogue Raw Start	
4 Analogue Raw End	
5 Send SMS	
6 Voltage for Battery full	
7 Cycle Loading Gel-Battery	
8 Cycle Loading Lead-Acid-Battery	
9 Maximum Voltage	
10 Language	
11 Battery-Type Gel-Type or Lead-Acid	
12 Channels Relay Solar	
13 Channels Load	
14 Sim-Karte Pin GSM-Modem
15 Battery full Hysteresis additional Device on
16 Umax -> add.Device on for x min/hr (0=off)	
17 Start / Stop Boost charge
18 Input-Nr for Simulation
19 Simulation-Value 
20 Generator	
21 PWM-charging	
22 Receive SMS	
23 Factor for Simulation by regulator	
24 Correction-Value for high Current Solar	
25 Time Boost charging To increase the	
26 Typ Analogue Input	
27 Number of universal channels in menu 1	
28 Number of NiCd/NimH-Cells	
29 NiCd/NimH Capacity	
30 Generator Start V/ SOC	
31 Start Generator at…	
32 Load switch off by V /SOC	
33 Correction SOC	
34 Adjust Solar Current	
35 Temp-Corr U Batt	
36 Rotate Y-Axis (vertical)	
37 Rotate Slip	
38 Time go back horizontal	
39 Amplifying factor horizontal tracking	
40 Running time Output  x	
41 Hardware-Version	
42 Solar charge on/off by Time	
43 with SD-Card (0/1)	
44 Scan Analogue Inputs (0-15)	
45 SD-Chip Block-Nr	
46 Dynamic Switch off Voltage-Level	
47 Analogue Input correction +/-	
48 Analogue Input correction Factor	
49 Number of Battery-Banks (0=off)	
50 Delay Battery Bank full (in min)	
51 U min->Switch to 1.Batt.Bank (0=off)	
52 Select Battery Bank manual	
53 Output (0-16) Battery full->Device on
54 Correction factor battery bank 2	
55 Correction river battery bank 3	
56 Correction solar current for not PWM charging	
57 Output (0-16) Start Motor
58 Output (0-16) Stop Motor
59 Output (0-16) Generator Load 
60 Output (0-16) Battery-Bank 1	
61 Output (0-16) Battery-Bank 2	
62 Output (0-16) Battery-Bank 3	
63 High Current Pulses on/off	
64 Network off / Master / Slave
65 Correction KWh (0,0…9,9)
66 Alarm at Start Generator (0/1)	 
67 Generator with Pre-Ignition
68 SOC Ah of the Battery
69 Correction Time	
70 Standard-Settings	
71 Correction Cable length	
72 Correction cable diameter	
73 NiCd or NimH	
74 Charge NiCd / NimH by Power-Mosfet	
75 Sending of logged Data to LogView	
76 Country-Code	
76 bistable Relay	
78 Phase Loop Control	
79 Message if the Battery is full	
80 Output X switches Output Y	
81 Output X switches Output Y	
82 Output X switches Output Y	
83 Output X switches Output Y	
84 Voltage Battery-Bank 1 off Output
85 Voltage Battery-Bank 2 off Output
86 Voltage Battery-Bank 3 off Output
87 Input Switch Battery-Bank 1 
88 Input Switch Battery-Bank 2
89 Input Switch Battery-Bank 3
90 Output Switch Battery-Bank 1 
91 Output Switch Battery-Bank 2
92 Output Switch Battery-Bank 3
93 Switch Battery-Bank on/off
94 94 Switch Output x by telephone
95 DCF77-Receiver for Date and Time
96 Number of Radio-Sensors
97 Number of digits_after comma
98 Switch off load at boost charge
99 Set-point detect night 
100 Reserve
101 Reserve
1 701 Battery voltage; 2 702 Output voltage
3 703 Moving-Detector; 4 704 Generator is running feedback
5 705 Temperature Solarpanels; '6 706 Temp 
7 707 Voltage Solar;8 708 Spare
9 709 Batt 2; 10 710 Batt 3
11 711 Load ext; 12 712 Load 2
13 713 Load 1; 14 714 I Solar
15 715 U NiCd; 16 716 Count 1
17 717 Count_2; 18 718 Freq_1
19 719 Freq_2; 20 720 Freq_2
1 721 Battery voltage;2 722 Output voltage
3 723 Moving-Detector;4 724 Generator is running feedback
5 725 Temperature Solarpanels;6 726 Temp 
7 727 'Voltage Solar;8 728 Res
9 729 Batt 2; 10 730 Batt 3
11 731 Load ext; 12 732 Load 2
13 733 Load 1;'14 734 I Solar
15 735 (U NiCd);'16 736 (Count 1)
17 737 (Count_2);'18 738 (Freq_1)
19 739 (Freq_2);'20 740 (Freq_2)
1 741 Battery voltage;'2 742 Output voltage
3 743 Moving-Detector;'4 744 Generator is running feedback
5 745 Temperature Solarpanels;'6 746 Temp
7 747 'Voltage Solar;'8 748 Res
9 749 Batt 2;'10 750 Batt 3
11 751 Load ext;'12 752 Load 2
13 753 Load 1;'14 754 I Solar
15 755 (U NiCd);'16 755 (Count 1)
17 756 (Count_2);'18 757 (Freq_1)
19 758 (Freq_2);'20 759 res 
