Parameters Irrigation System																		
Nr
1 Correction cable length (only for Solar charge controller)	
2 Correction Cable Area (only for Solar charge controller)	
3 Days without watering	
4 Voltage for Pre-warning (only for Solar charge controller)	
5 Hysteresis (only for Solar charge controller)	
6 Voltage for Battery full (only for Solar charge controller)	
7 Cycle Loading Gel-Battery (only for Solar charge controller)	
8 Cycle Loading Lead-Acid-Battery (only for Solar charge controller)	
9 Maximum Voltage (only for Solar charge controller)	
10 Language	
11 Battery-Type Gel or not (only for Solar charge controller)	
12 Irrigation Average-Calculation	
13 Number of Channels	
14 Correction Time	
15 Sensor-Type	
16 Analogue Correction +/-	
17 Analogue Correction x	
18 Sending of logged Data to LogView	
19 Factory Settings	
20 latching relay	
21 Minimum switch on / off time	
22 Receive SMS	
23 Send SMS	25
23 Country Code for SMS	
25 Alarm at  Cable-Break	
26 Auto-Detect Min/Max Humidity;	
27 Type of Radio-Sensor	
28 Number of NiCd/NimH / on/off	
29 NiCd/NimH Capacity	
30 Solar-Charger active (only for Solar charge controller)	
31 Scan-Time Data-Logging	
32 correction of irrigation-time depending from the ambient temperature	
33 Solar Thermal System?
34 Solar I Correction (Solar charge controller)	
35 Temp-Correction U Battery (only for Solar charge controller)	
36 PWM-charging (only for Solar charge controller)	
37 Max.Time for Anti-Frost-Irrigation	
38 Caculation Enthalpie, Flow-calculation
39 Correction Counter (f.e. KWh-Counter)	
40 Scan counter 1 and 2
41 Hardware-Version
42 Zones Universal-Modul	
43 Start/Stop Boost-charge (only for Solar charge controller)	
44 with SD-Card (0/1)	
45 Number of Scans Analogue Inputs (0-15)	
46 SD-Chip Block-Nr
47 Load 1 Select Output	
48 Load 2 Select Output	
49 Load 3 Select Output	
50 Load 4 Select Output	
51 Load 5 Select Output	
52 Analogue Range Start	
53 Analogue Range End	
54 Analogue Raw Start	
55 Analogue Raw End	
56 Parameter-Number for Simu	
57 Simu-Value
58 Simulation by Regulator	
59 Pulsed Output on-Pulse	
60 Pulsed Output off-Pulse	
61 Pulsed Output on-Pulse	
62 Pulsed Output off-Pulse	
63 Pulsed Output on-Pulse	
64 Pulsed Output off-Pulse	
65 Pulsed Output on-Pulse	
66 Pulsed Output off-Pulse	
67 Antiblocking-System Output x
68 Antiblocking-System Output x
69 Antiblocking-System Output x
70 Antiblocking-System Output x
71 Antiblocking-System Output x
72 Minimum-Value Analog-Input	
73 Maximal-Value Analog-Input	
74 Running-Time Output x	
74 Running-Time Output x	
75 Output X switches Output Y	
76 Output X switches Output Y	
77 Output X switches Output Y	
78 Output X switches Output Y	
79 Reserve
80 Reserve
81 Reserve
82 Reserve
83 Reserve
84 Reserve
85 Reserve
1 701 Type Battery voltage; '2 702 Output voltage
3 703 Type Sensor 3; '4 704 Sensor 4             
5 705 Type Sensor 5; '6 706 Sensor 6             
7 707 Type Sensor 7;8 708 Spare                  
9 709 Type Batt 2; 10 710 Batt 3                 
11 711 Type Load ext; 12 712 Load 2              
13 713 Type Load 1; 14 714 I Solar               
15 715 Type U NiCd; 16 716 Count 1               
17 717 Type Count_2; 18 718 Freq_1               
19 719 Type Freq_2; 20 720 Freq_2                
1 721 +/- Battery voltage;2 722 Output voltage   
3 723 +/- Sensor 3;4 724 Sensor 4                
5 725 +/- Sensor 5;6 726 Sensor 6                
7 727 +/- Sensor 7;8 728 Res                     
9 729 +/- Batt 2; 10 730 Batt 3                  
11 731 +/-Load ext; 12 732 Load 2                
13 733 +/-Load 1;'14 734 I Solar                 
15 735 +/-(U NiCd);'16 736 (Count 1)             
17 737 +/-(Count_2);'18 738 (Freq_1)             
19 739 +/-(Freq_2);'20 740 (Freq_2)              
1 741 * Battery voltage;'2 742 Output voltage    
3 743 * Sensor 3;'4 744 Sensor 4                 
5 745 * Sensor 5;'6 746 Sensor 6                 
7 747 * Sensor 7;'8 748 Res                      
9 749 * Batt 2;'10 750 Batt 3                    
11 751 * Load ext;'12 752 Load 2                 
13 753 * Load 1;'14 754 I Solar                  
15 755 * (U NiCd);'16 755 (Count 1)              
17 756 * (Count_2);'18 757 (Freq_1)              
19 758 * (Freq_2);'20 759 res                    
                                                 
