OVerview universal-Channels
No
1.Channel Function________________ Timer hour 
1.Channel Timer minute
1.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
1.Channel Pulse all.. (< 100=min / > 100=Std / > 200=days)
1.Channel Setvalue 
1.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
1.Channel actual value > / < Setvalue (0 = < /1 = >)
1.Channel hysteresis (difference On/Off Setvalue/ actual value)
2.Channel Function________________ Timer hour 
2.Channel Timer minute
2.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
2.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
2.Channel Setvalue 
2.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
2.Channel actual value > / < Setvalue (0 = < /1 = >)
2.Channel hysteresis (difference On/Off Setvalue/ actual value)
3.Channel Function________________ Timer hour 
3.Channel Timer minute
3.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
3.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
3.Channel Setvalue 
3.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
3.Channel actual value > / < Setvalue (0 = < /1 = >)
3.Channel hysteresis (difference On/Off Setvalue/ actual value)
4.Channel Function________________ Timer hour 
4.Channel Timer minute
4.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
4.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
4.Channel Setvalue 
4.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
4.Channel actual value > / < Setvalue (0 = < /1 = >)
4.Channel hysteresis (difference On/Off Setvalue/ actual value)
5.Channel Function________________ Timer hour 
5.Channel Timer minute
5.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
5.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
5.Channel Setvalue 
5.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
5.Channel actual value > / < Setvalue (0 = < /1 = >)
5.Channel hysteresis (difference On/Off Setvalue/ actual value)
6.Channel Function________________ Timer hour 
6.Channel Timer minute
6.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
6.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
6.Channel Setvalue 
6.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
6.Channel actual value > / < Setvalue (0 = < /1 = >)
6.Channel hysteresis (difference On/Off Setvalue/ actual value)
7.Channel Function________________ Timer hour 
7.Channel Timer minute
7.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
7.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
7.Channel Setvalue 
7.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
7.Channel actual value > / < Setvalue (0 = < /1 = >)
7.Channel hysteresis (difference On/Off Setvalue/ actual value)
8.Channel Function________________ Timer hour 
8.Channel Timer minute
8.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
8.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
8.Channel Setvalue 
8.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
8.Channel actual value > / < Setvalue (0 = < /1 = >)
8.Channel hysteresis (difference On/Off Setvalue/ actual value)
9.Channel Function________________ Timer hour 
9.Channel Timer minute
9.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
9.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
9.Channel Setvalue 
9.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
9.Channel actual value > / < Setvalue (0 = < /1 = >)
9.Channel hysteresis (difference On/Off Setvalue/ actual value)
10.Channel Function________________ Timer hour 
10.Channel Timer minute
10.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
10.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
10.Channel Setvalue 
10.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
10.Channel actual value > / < Setvalue (0 = < /1 = >)
10.Channel hysteresis (difference On/Off Setvalue/ actual value)
11.Channel Function________________ Timer hour 
11.Channel Timer minute
11.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
11.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
11.Channel Setvalue 
11.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
11.Channel actual value > / < Setvalue (0 = < /1 = >)
11.Channel hysteresis (difference On/Off Setvalue/ actual value)
12.Channel Function________________ Timer hour 
12.Channel Timer minute
12.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
12.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
12.Channel Setvalue 
12.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
12.Channel actual value > / < Setvalue (0 = < /1 = >)
12.Channel hysteresis (difference On/Off Setvalue/ actual value)
13.Channel Function________________ Timer hour 
13.Channel Timer minute
13.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
13.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
13.Channel Setvalue 
13.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
13.Channel actual value > / < Setvalue (0 = < /1 = >)
13.Channel hysteresis (difference On/Off Setvalue/ actual value)
14.Channel Function________________ Timer hour 
14.Channel Timer minute
14.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
14.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
14.Channel Setvalue 
14.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
14.Channel actual value > / < Setvalue (0 = < /1 = >)
14.Channel hysteresis (difference On/Off Setvalue/ actual value)
15.Channel Function________________ Timer hour 
15.Channel Timer minute
15.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
15.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
15.Channel Setvalue 
15.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
15.Channel actual value > / < Setvalue (0 = < /1 = >)
15.Channel hysteresis (difference On/Off Setvalue/ actual value)
16.Channel Function________________ Timer hour 
16.Channel Timer minute
16.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
16.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
16.Channel Setvalue 
16.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
16.Channel actual value > / < Setvalue (0 = < /1 = >)
16.Channel hysteresis (difference On/Off Setvalue/ actual value)
17.Channel Function________________ Timer hour 
17.Channel Timer minute
17.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
17.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
17.Channel Setvalue 
17.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
17.Channel actual value > / < Setvalue (0 = < /1 = >)
17.Channel hysteresis (difference On/Off Setvalue/ actual value)
18.Channel Function________________ Timer hour 
18.Channel Timer minute
18.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
18.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
18.Channel Setvalue 
18.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
18.Channel actual value > / < Setvalue (0 = < /1 = >)
18.Channel hysteresis (difference On/Off Setvalue/ actual value)
19.Channel Function________________ Timer hour 
19.Channel Timer minute
19.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
19.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
19.Channel Setvalue 
19.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
19.Channel actual value > / < Setvalue (0 = < /1 = >)
19.Channel hysteresis (difference On/Off Setvalue/ actual value)
20.Channel Function________________ Timer hour 
20.Channel Timer minute
20.Channel Pulse active-Time (< 100=sec / > 100=min / > 200=hr)
20.Channel Pulse all.. (< 100=min / > 100=hr / > 200=days)
20.Channel Setvalue 
20.Channel time Active-Time (< 100=sec / > 100=min / > 200=hr)
20.Channel actual value > / < Setvalue (0 = < /1 = >)
20.Channel hysteresis (difference On/Off Setvalue/ actual value)
1.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204
1.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)
1.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding
1.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp
1.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp
1.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr) 
1.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)
1.Channel Delay off (< 100=sec / > 100=min / > 200=hr)
1.Channel On (on=1/Off=0)
1.Channel Input 2 O.K. = 0 or 1?
2.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
2.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
2.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
2.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
2.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
2.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
2.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
2.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
2.Channel On (on=1/Off=0)                                                                              
2.Channel Input 2 O.K. = 0 or 1?                                                                       
3.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
3.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
3.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
3.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
3.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
3.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
3.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
3.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
3.Channel On (on=1/Off=0)                                                                              
3.Channel Input 2 O.K. = 0 or 1?                                                                       
4.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
4.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
4.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
4.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
4.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
4.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
4.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
4.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
4.Channel On (on=1/Off=0)                                                                              
4.Channel Input 2 O.K. = 0 or 1?                                                                       
5.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
5.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
5.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
5.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
5.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
5.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
5.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
5.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
5.Channel On (on=1/Off=0)                                                                              
5.Channel Input 2 O.K. = 0 or 1?                                                                       
6.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
6.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
6.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
6.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
6.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
6.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
6.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
6.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
6.Channel On (on=1/Off=0)                                                                              
6.Channel Input 2 O.K. = 0 or 1?                                                                       
7.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
7.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
7.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
7.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
7.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
7.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
7.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
7.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
7.Channel On (on=1/Off=0)                                                                              
7.Channel Input 2 O.K. = 0 or 1?                                                                       
8.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
8.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
8.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
8.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
8.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
8.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
8.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
8.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
8.Channel On (on=1/Off=0)                                                                              
8.Channel Input 2 O.K. = 0 or 1?                                                                       
9.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
9.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
9.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
9.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
9.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
9.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
9.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
9.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
9.Channel On (on=1/Off=0)                                                                              
9.Channel Input 2 O.K. = 0 or 1?                                                                       
10.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204  
10.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)     
10.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding   
10.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
10.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp         
10.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                    
10.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                      
10.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                 
10.Channel On (on=1/Off=0)                                                                              
10.Channel Input 2 O.K. = 0 or 1?                                                                       
11.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
11.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
11.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
11.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
11.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
11.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
11.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
11.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
11.Channel On (on=1/Off=0)                                                                                 
11.Channel Input 2 O.K. = 0 or 1?                                                                          
12.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
12.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
12.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
12.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
12.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
12.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
12.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
12.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
12.Channel On (on=1/Off=0)                                                                                 
12.Channel Input 2 O.K. = 0 or 1?                                                                          
13.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
13.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
13.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
13.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
13.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
13.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
13.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
13.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
13.Channel On (on=1/Off=0)                                                                                 
13.Channel Input 2 O.K. = 0 or 1?                                                                          
14.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
14.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
14.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
14.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
14.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
14.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
14.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
14.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
14.Channel On (on=1/Off=0)                                                                                 
14.Channel Input 2 O.K. = 0 or 1?                                                                          
15.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
15.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
15.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
15.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
15.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
15.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
15.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
15.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
15.Channel On (on=1/Off=0)                                                                                 
15.Channel Input 2 O.K. = 0 or 1?                                                                          
16.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
16.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
16.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
16.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
16.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
16.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
16.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
16.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
16.Channel On (on=1/Off=0)                                                                                 
16.Channel Input 2 O.K. = 0 or 1?                                                                          
17.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
17.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
17.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
17.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
17.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
17.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
17.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
17.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
17.Channel On (on=1/Off=0)                                                                                 
17.Channel Input 2 O.K. = 0 or 1?                                                                          
18.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
18.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
18.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
18.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
18.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
18.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
18.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
18.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
18.Channel On (on=1/Off=0)                                                                                 
18.Channel Input 2 O.K. = 0 or 1?                                                                          
19.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
19.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
19.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
19.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
19.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
19.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
19.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
19.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
19.Channel On (on=1/Off=0)                                                                                 
19.Channel Input 2 O.K. = 0 or 1?                                                                          
20.Channel function ________________ Input 1 (analogue Input). 1-15; Digital Inp.01-108; Radio 201-204     
20.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)        
20.Channel type (0=%; 1=°C; 2 =%; 3=V; 5=A;10=Alarm;from 20=Interlock;from 30=Impuls;40=load Shedding      
20.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
20.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp            
20.Channel Max.Time Output active (< 100=sec / > 100=min / > 200=hr)                                       
20.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=hr)                                         
20.Channel Delay off (< 100=sec / > 100=min / > 200=hr)                                                    
20.Channel On (on=1/Off=0)                                                                                 
20.Channel Input 2 O.K. = 0 or 1?                                                                          
1.Channel Automatic calculation irrigation-Time (0=off/1=on)
2.Channel Automatic calculation irrigation-Time (0=off/1=on)
3.Channel Automatic calculation irrigation-Time (0=off/1=on)
4.Channel Automatic calculation irrigation-Time (0=off/1=on)
5.Channel Automatic calculation irrigation-Time (0=off/1=on)
6.Channel Automatic calculation irrigation-Time (0=off/1=on)
7.Channel Automatic calculation irrigation-Time (0=off/1=on)
8.Channel Automatic calculation irrigation-Time (0=off/1=on)
9.Channel Automatic calculation irrigation-Time (0=off/1=on)
10.Channel Automatic calculation irrigation-Time (0=off/1=on)
11.Channel Automatic calculation irrigation-Time (0=off/1=on)
12.Channel Automatic calculation irrigation-Time (0=off/1=on)
13.Channel Automatic calculation irrigation-Time (0=off/1=on)
14.Channel Automatic calculation irrigation-Time (0=off/1=on)
15.Channel Automatic calculation irrigation-Time (0=off/1=on)
16.Channel Automatic calculation irrigation-Time (0=off/1=on)
17.Channel Automatic calculation irrigation-Time (0=off/1=on)
18.Channel Automatic calculation irrigation-Time (0=off/1=on)
19.Channel Automatic calculation irrigation-Time (0=off/1=on)
20.Channel Automatic calculation irrigation-Time (0=off/1=on)
1.Channel next alarm in x min
2.Channel next alarm in x min
3.Channel next alarm in x min
4.Channel next alarm in x min
5.Channel next alarm in x min
6.Channel next alarm in x min
7.Channel next alarm in x min
8.Channel next alarm in x min
9.Channel next alarm in x min
10.Channel next alarm in x min
11.Channel next alarm in x min
12.Channel next alarm in x min
13.Channel next alarm in x min
14.Channel next alarm in x min
15.Channel next alarm in x min
16.Channel next alarm in x min
17.Channel next alarm in x min
18.Channel next alarm in x min
19.Channel next alarm in x min
20.Channel next alarm in x min
1.Channel alarm no flow after x min (detect by change of actual value); 0=off
2.Channel alarm no flow after x min (detect by change of actual value); 0=off
3.Channel alarm no flow after x min (detect by change of actual value); 0=off
4.Channel alarm no flow after x min (detect by change of actual value); 0=off
5.Channel alarm no flow after x min (detect by change of actual value); 0=off
6.Channel alarm no flow after x min (detect by change of actual value); 0=off
7.Channel alarm no flow after x min (detect by change of actual value); 0=off
8.Channel alarm no flow after x min (detect by change of actual value); 0=off
9.Channel alarm no flow after x min (detect by change of actual value); 0=off
10.Channel alarm no flow after x min (detect by change of actual value); 0=off
11.Channel alarm no flow after x min (detect by change of actual value); 0=off
12.Channel alarm no flow after x min (detect by change of actual value); 0=off
13.Channel alarm no flow after x min (detect by change of actual value); 0=off
14.Channel alarm no flow after x min (detect by change of actual value); 0=off
15.Channel alarm no flow after x min (detect by change of actual value); 0=off
16.Channel alarm no flow after x min (detect by change of actual value); 0=off
17.Channel alarm no flow after x min (detect by change of actual value); 0=off
18.Channel alarm no flow after x min (detect by change of actual value); 0=off
19.Channel alarm no flow after x min (detect by change of actual value); 0=off
20.Channel alarm no flow after x min (detect by change of actual value); 0=off
