Overview universal-Channel Solar
No
1.channel function....... Timers hour 
1.channel Timer minute
1.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
1.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
1.channel Set-value 
1.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
1.channel actual value > / < Setvalue (0 = < /1 = >)
1.channel hysteresis
2.channel function....... Timer hour 
2.channel Timer minute
2.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
2.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
2.channel Setvalue 
2.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
2.channel actual value > / < Setvalue (0 = < /1 = >)
2.channel hysteresis
3.channel function....... Timer hour 
3.channel Timer minute
3.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
3.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
3.channel Setvalue 
3.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
3.channel actual value > / < Setvalue (0 = < /1 = >)
3.channel hysteresis
4.channel function....... Timer hour 
4.channel Timer minute
4.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
4.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
4.channel Setvalue 
4.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
4.channel actual value > / < Setvalue (0 = < /1 = >)
4.channel hysteresis
5.channel function....... Timer hour 
5.channel Timer minute
5.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
5.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
5.channel Setvalue 
5.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
5.channel actual value > / < Setvalue (0 = < /1 = >)
5.channel hysteresis
6.channel function....... Timer hour 
6.channel Timer minute
6.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
6.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
6.channel Setvalue 
6.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
6.channel actual value > / < Setvalue (0 = < /1 = >)
6.channel hysteresis
7.channel function....... Timer hour 
7.channel Timer minute
7.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
7.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
7.channel Setvalue 
7.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
7.channel actual value > / < Setvalue (0 = < /1 = >)
7.channel hysteresis
8.channel function....... Timer hour 
8.channel Timer minute
8.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
8.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
8.channel Setvalue 
8.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
8.channel actual value > / < Setvalue (0 = < /1 = >)
8.channel hysteresis
9.channel function....... Timer hour 
9.channel Timer minute
9.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
9.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
9.channel Setvalue 
9.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
9.channel actual value > / < Setvalue (0 = < /1 = >)
9.channel hysteresis
10.channel function....... Timer hour 
10.channel Timer minute
10.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
10.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
10.channel Setvalue 
10.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
10.channel actual value > / < Setvalue (0 = < /1 = >)
10.channel hysteresis
11.channel function....... Timer hour 
11.channel Timer minute
11.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
11.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
11.channel Setvalue 
11.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
11.channel actual value > / < Setvalue (0 = < /1 = >)
11.channel hysteresis
12.channel function....... Timer hour 
12.channel Timer minute
12.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
12.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
12.channel Setvalue 
12.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
12.channel actual value > / < Setvalue (0 = < /1 = >)
12.channel hysteresis
13.channel function....... Timer hour 
13.channel Timer minute
13.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
13.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
13.channel Setvalue 
13.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
13.channel actual value > / < Setvalue (0 = < /1 = >)
13.channel hysteresis
14.channel function....... Timer hour 
14.channel Timer minute
14.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
14.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
14.channel Setvalue 
14.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
14.channel actual value > / < Setvalue (0 = < /1 = >)
14.channel hysteresis
15.channel function....... Timer hour 
15.channel Timer minute
15.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
15.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
15.channel Setvalue 
15.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
15.channel actual value > / < Setvalue (0 = < /1 = >)
15.channel hysteresis
16.channel function....... Timer hour 
16.channel Timer minute
16.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
16.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
16.channel Setvalue 
16.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
16.channel actual value > / < Setvalue (0 = < /1 = >)
16.channel hysteresis
17.channel function....... Timer hour 
17.channel Timer minute
17.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
17.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
17.channel Setvalue 
17.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
17.channel actual value > / < Setvalue (0 = < /1 = >)
17.channel hysteresis
18.channel function....... Timer hour 
18.channel Timer minute
18.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
18.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
18.channel Setvalue 
18.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
18.channel actual value > / < Setvalue (0 = < /1 = >)
18.channel hysteresis
19.channel function....... Timer hour 
19.channel Timer minute
19.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
19.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
19.channel Setvalue 
19.channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
19.channel actual value > / < Setvalue (0 = < /1 = >)
19.channel hysteresis
20.channel function....... Timer hour 
20.channel Timer minute
20.channel Pulse active-Time (< 100=sec / > 100=min / > 200=Std)
20.channel Pulse all.. (< 100=min / > 100=Std / > 200=Tage)
20.Channel Setvalue 
20.Channel time Active-Time (< 100=sec / > 100=min / > 200=Std)
20.Channel actual value > / < Setvalue (0 = < /1 = >)
20.Channel hysteresis
1.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204
1.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)
1.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding
1.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp
1.Channel Input 2 O.K. = 0 or 1?
1.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp
1.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)
1.Channel Delay off (< 100=sec / > 100=min / > 200=Std)
1.Channel On (on=1 / Off=0)
1.Channel delay time next alarm 
2.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
2.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
2.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
2.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
2.Channel Input 2 O.K. = 0 or 1?                                                                                      
2.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
2.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
2.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
2.Channel On (on=1 / Off=0)                                                                                           
2.Channel delay time next alarm                                                                                       
3.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
3.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
3.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
3.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
3.Channel Input 2 O.K. = 0 or 1?                                                                                      
3.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
3.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
3.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
3.Channel On (on=1 / Off=0)                                                                                           
3.Channel delay time next alarm                                                                                       
4.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
4.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
4.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
4.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
4.Channel Input 2 O.K. = 0 or 1?                                                                                      
4.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
4.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
4.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
4.Channel On (on=1 / Off=0)                                                                                           
4.Channel delay time next alarm                                                                                       
5.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
5.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
5.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
5.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
5.Channel Input 2 O.K. = 0 or 1?                                                                                      
5.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
5.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
5.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
5.Channel On (on=1 / Off=0)                                                                                           
5.Channel delay time next alarm                                                                                       
6.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
6.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
6.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
6.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
6.Channel Input 2 O.K. = 0 or 1?                                                                                      
6.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
6.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
6.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
6.Channel On (on=1 / Off=0)                                                                                           
6.Channel delay time next alarm                                                                                       
7.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
7.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
7.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
7.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
7.Channel Input 2 O.K. = 0 or 1?                                                                                      
7.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
7.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
7.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
7.Channel On (on=1 / Off=0)                                                                                           
7.Channel delay time next alarm                                                                                       
8.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
8.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
8.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
8.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
8.Channel Input 2 O.K. = 0 or 1?                                                                                      
8.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
8.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
8.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
8.Channel On (on=1 / Off=0)                                                                                           
8.Channel delay time next alarm                                                                                       
9.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
9.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
9.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
9.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
9.Channel Input 2 O.K. = 0 or 1?                                                                                      
9.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
9.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
9.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
9.Channel On (on=1 / Off=0)                                                                                           
9.Channel delay time next alarm                                                                                       
10.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
10.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
10.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
10.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
10.Channel Input 2 O.K. = 0 or 1?                                                                                      
10.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
10.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
10.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
10.Channel On (on=1 / Off=0)                                                                                           
10.Channel delay time next alarm                                                                                       
11.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                     
11.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                    
11.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding  
11.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                       
11.Channel Input 2 O.K. = 0 or 1?                                                                                      
11.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                        
11.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                    
11.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                               
11.Channel On (on=1 / Off=0)                                                                                           
11.Channel delay time next alarm                                                                                       
12.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                       
12.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                      
12.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding    
12.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                         
12.Channel Input 2 O.K. = 0 or 1?                                                                                        
12.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                          
12.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                      
12.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                 
12.Channel On (on=1 / Off=0)                                                                                             
12.Channel delay time next alarm                                                                                         
13.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                       
13.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                      
13.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding    
13.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                         
13.Channel Input 2 O.K. = 0 or 1?                                                                                        
13.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                          
13.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                      
13.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                 
13.Channel On (on=1 / Off=0)                                                                                             
13.Channel delay time next alarm                                                                                         
14.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                       
14.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                      
14.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding    
14.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                         
14.Channel Input 2 O.K. = 0 or 1?                                                                                        
14.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                          
14.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                      
14.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                 
14.Channel On (on=1 / Off=0)                                                                                             
14.Channel delay time next alarm                                                                                         
15.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                       
15.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                      
15.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding    
15.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                         
15.Channel Input 2 O.K. = 0 or 1?                                                                                        
15.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                          
15.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                      
15.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                 
15.Channel On (on=1 / Off=0)                                                                                             
15.Channel delay time next alarm                                                                                         
16.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                            
16.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                           
16.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding         
16.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                              
16.Channel Input 2 O.K. = 0 or 1?                                                                                             
16.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                               
16.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                           
16.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                      
16.Channel On (on=1 / Off=0)                                                                                                  
16.Channel delay time next alarm                                                                                              
17.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                            
17.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                           
17.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding         
17.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                              
17.Channel Input 2 O.K. = 0 or 1?                                                                                             
17.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                               
17.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                           
17.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                      
17.Channel On (on=1 / Off=0)                                                                                                  
17.Channel delay time next alarm                                                                                              
18.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                            
18.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                           
18.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding         
18.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                              
18.Channel Input 2 O.K. = 0 or 1?                                                                                             
18.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                               
18.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                           
18.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                      
18.Channel On (on=1 / Off=0)                                                                                                  
18.Channel delay time next alarm                                                                                              
19.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                            
19.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                           
19.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding         
19.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                              
19.Channel Input 2 O.K. = 0 or 1?                                                                                             
19.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                               
19.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                           
19.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                      
19.Channel On (on=1 / Off=0)                                                                                                  
19.Channel delay time next alarm                                                                                              
20.Channel function........... Input 1 (analogue Input). 1-15; Digital Inp. 101-108; Radio 201-204                            
20.Channel Input 2 (Interlock Outp). 1-20; Analogue Inp.51-66; Digital Inp.101-108; Radio 201 -204)                           
20.Channel type (V=0);°C=1; %=2; A=3;5=Gen.Start;from 10=Alarm;from 20=Interlock;from 30=Impuls;from 40=load Shedding         
20.Channel Output 1 (2-7= relay; 1 u.8-14=transistor; 15=Relaiy NimH; 16=Teleph; 17-20=virt.Outp                              
20.Channel Input 2 O.K. = 0 or 1?                                                                                             
20.Channel Output 2 (2-7= relay; 1 u.8-14=transistor; 15=Relay NimH; 16=Teleph; 17-20=virt.Outp                               
20.Channel Delay on Act </> Set (< 100=sec / > 100=min / > 200=Std)                                                           
20.Channel Delay off (< 100=sec / > 100=min / > 200=Std)                                                                      
20.Channel On (on=1 / Off=0)                                                                                                  
20.Channel delay time next alarm                                                                                              
